1. Decompress the software first
2. Install the "NetFx20SP2_x86" software first, after that, please double click the software"eMaxim_link_tool"
3. Connect with the receiver to your PC, and turn on the mouse(need to install the battery).
4. After you open the software "eMaxim_link_tool'', please click the "find my device", if it show green mark (link), the mouse can work. If it show unlink, then please click verify code, the device will match the code automatically(about 20 seconds it can be finished). 
5. If you still can not unlink, you can change the Product ID(hex) 0001 to AC01 and try it again.



  



使用说明:

使用本软件之前请
文件进行对吗。
1.	解压 <亿美国际对码工具包.rar>

2.	先安装NetFx20SP2_x86系统文件，安装成功之后运行eMaxim_link_tool，双击打开eMaxim_link_tool

3.	插入接收器点击<Find My Device>等待Connect:显示Link. 如显示unLink,请将Product ID 改为AC01再试


4.	点击<Verify Code>按钮,LED将会闪烁20秒,　同时按鼠标的左中右三个键可进行配对,　配对成功LED熄灭。如果依然无法配对，及时接收头或者鼠标有故障。






使用本软件请注意将 <设备管理器>-<硬件>-<通用串行总线控制器>-<USB Root Hub属性>-<电源管理>-<允许计算机关闭这个设备以节约电源> 这个选项取消

	

